## Doors

#### Front Door Panel Removal/Installation (cont'd)

20-8

Front door Outer Handle Replacement

6. Release the clips that hold the door panel (A) with a commercially available trim pad remover (B), then remove the door panel by pulling it upward. Passenger's door: Disconnect the power window switch connector (for some models). Remove the door panel with as little bending as possible to avoid creasing or breaking it.

   Fastener Locations
   : Clip, 7

7. Install the door panel in the reverse order of removal, and note these items:

- Replace any damaged clips.
- Make sure the connectors are plugged in properly, and the rod is connected properly.
- If applicable, install the regulator handle so it points forward and up at a 45° angle with the glass fully closed.

NOTE: Put on gloves to protect your hands.

1. Raise the glass fully.
2. Remove these items:

- Door panel (see page 20-7)
- Plastic cover, as necessary (see page 20-3)

3. Release the retainer clip (A), then remove the lock cylinder (B). Disconnect the cylinder rod (C).

4. With cylinder switch: Remove the screw, then separate the lock cylinder (A) and cylinder switch (B).

   Fastener Location
   : Screw, 1