## EPS Components

#### Steering Gearbox Installation

17-21

NOTE: RHD type is shown, LHD type is symmetrical.

1. Before installing the gearbox, slide the rack all the way to the passenger's side (RHD: left direction, LHD: right direction).

1. Pass the passenger's side of the steering gearbox together with the tie-rods through the wheel well opening on the passenger's side. Continue moving the steering gearbox toward the passenger's side until the driver's side rack end clears the master cylinder. Lower the driver's side (pinion side) of the steering gearbox and back it toward the driver's side until the steering gearbox is in position.

1. Install the heater valve (A) on the bulkhead. Through the heater valve cable (B) into the canister bracket and connect the heater valve cable end to the heater valve arm (C). Close the cable clamp.

1. Hold the coolant hose (D) on the hose holders.

1. Install the coolant expansion tank (A) and canister bracket (B).

a a a