## Interior Trim

#### Trim Removal/Installation - Door Area

20-206

NOTE:

- Put on gloves to protect your hands.
- When prying with a flat-tip screwdriver, wrap it with protective tape to prevent damage.
- Take care not to bend or scratch the trim and panels.

Remove the trim as shown. To remove the rear door sill trim, remove the seat side trim (see page 20-207).

Install the trim in the reverse order of removal and note these items:

- Replace any damaged clips.
- Apply liquid thread lock to the front seat belt upper anchor bolt before installation.
- Before installing the anchor bolts, make sure there are no twists or kinks in the belts.

  Fastener Locations
  A : Clip, 2 (Black) | B : Clip, 3 (White) | C : Clip, 9
  1. FRONT PILLAR TRIM
  2. FRONT DOOR OPENING TRIM
  3. FRONT SEAT BELT UPPER ANCHOR BOLT, 7/16-20 UNF, 32 Nm (3.3 kgf m, 24 lbf ft)
  4. CENTRE PILLAR UPPER TRIM
  5. REAR DOOR OPENING TRIM
  6. SEAT SIDE TRIM
  7. REAR DOOR SILL TRIM
  8. FRONT SEAT BELT UPPER ANCHOR BOLT, 7/16-20 UNF, 32 Nm (3.3 kgf m, 24 lbf ft)
  9. HOOK
  10. FRONT SIDE CAP
  11. HOOK
  12. HOOKS
  13. KICK PANEL
  14. FRONT DOOR SILL TRIM
  15. CENTRE PILLAR LOWER TRIM
  16. UPPER ANCHOR COVER