## Transmission End Cover

#### Park Lever Stop Inspection and Adjustment

14-174

1. Set the park lever in the position.

2. Measure the distance (A) between the park pawl shaft (B) and the park lever roller pin (C).

STANDARD:

72.9-73.9 mm (2.87-2.91 in.)

3. If the measurement is out of tolerance, select and install the appropriate park lever stop (A) from the table below.

PARK LEVER STOP

Mark | Part Number | L1 | L2
1 | 24537-PA9-003 | 11.00 mm (0.433 in.) | 11.00 mm (0.433 in.)
2 | 24538-PA9-003 | 10.80 mm (0.425 in.) | 10.65 mm (0.419 in.)
3 | 24539-PA9-003 | 10.60 mm (0.417 in.) | 10.30 mm (0.406 in.)

4. After replacing the park lever stop, make sure the distance is within tolerance.