## Interior Trim

#### Trim Removal/Installation - Rear Shelf Area - Folding Type Rear Seat

20-65

NOTE:

- Put on gloves to protect your hands.
- When prying with a flat-tip screwdriver, wrap it with protective tape to prevent damage.
- Take care not to bend or scratch the trim and panels.

Remove the trim as shown. To remove the rear shelf, remove the rear seat side bolster from each side (see page 20-95), lock cylinder trim (see step 1 on page 20-97), and child seat tether anchor fitting (see page 23-12) (KQ model).

Install the trim in the reverse order of removal, and note these items:

- Replace any damaged clips.
- When installing the rear shelf, slip the rear seat belts and centre belt through the slits and hole in the rear shelf.
- Make sure the high mount brake light connector is plugged in properly.

  Fastener Locations
  A : Clip, 5 (White) | B : Clip, 2 | C : Clip, 12
  1. BODY
  2. HOOK
  3. REAR SHELF
  4. HOOK
  5. LOCK CYLINDER TRIM
  6. CENTRE RETRACTOR CAP
  7. REAR WINDOW DEFOGGER HARNESS
  8. REAR PILLAR TRIM
  9. SLIT
  10. REAR DOOR OPENING TRIM
  11. SEAT SIDE TRIM
  12. REAR SEAT BELT
  13. REAR CENTRE BELT

      (For some models)

  14. REAR CENTRE BELT CENTRE ANCHOR BOLT

      7/16-20 UNF, 32 Nm (3.3 kgf m, 24 lbf ft)

  15. HIGH MOUNT BRAKE LIGHT CONNECTOR
  16. REAR SHELF
  17. REAR SEAT BELT
  18. SLIT
  19. HOOK