## Sunroof

#### Motor Test

22-158
Limit Switch Test

1. Remove the headliner (see page 20-68).

2. Disconnect the 2P connector from the sunroof motor.

3. Check the motor by connecting power and ground according to the table.

4. If the motor does not run, replace it.
   NOTE: See closing force check (see page 20-62) for motor clutch test.

1. Remove the headliner (see page 20-68).

2. Disconnect the 4P connector from the sunroof limit switch.

Terminal side of male terminal

3. Check for continuity between the terminals in each switch position according to the table.
   NOTE: Turn the motor by hand with the wrench.

4. If there is no continuity, replace the cable assembly.