## Seat Belts

#### Front Seat Belt Replacement

23-2

SRS components are located in this area. Review the SRS component location, precautions and procedures in the SRS section before performing repairs or service. Refer to the '01 Civic Shop Manual on this CD, P/N 62S5A00. NOTE: Check the front seat belts for damage and replace them if necessary. Be careful not to damage them during removal and installation.

Front Seat Belt

1. Disconnect the negative battery cable and wait at least 3 minutes before beginning work.
2. Slide the front seat forward fully.
3. Remove the lower anchor bolts, then remove the slide bar (A).

4. Remove the rear side trim panel (see page 20-30).

5. Remove the upper anchor cover (A), and remove the upper anchor bolt (B).

6. Disconnect the seat belt tensioner connector (A). Remove the retractor mounting self-tapping ET screw (B) and the retractor bolt (C), then remove the front seat belt (D) and retractor (E).

a a a