## Seat Belts

#### Front Seat Belt Replacement (cont'd)

23-7

Seat Belt Buckle

1. If equipped, make sure you have the anti-theft code for the radio, then write down the frequencies for the preset buttons.
2. If equipped, with a side airbag disconnect the negative battery cable, and wait at least 3 minutes before beginning work.
3. Remove the front seat (see page 20-87).
4. Remove the centre cover from the seat, with manual height adjustable (see page 20-89), without manual height adjustable (see page 20-90).
5. On the driver's seat for some models, detach the seat belt switch connector (A) and harness clip (B). LHD is shown, RHD is symmetrical.

With manual height adjustable:

Without manual height adjustable:

6. With manual height adjustable, adjust the seat cushion to its maximum height.

7. Remove the centre anchor bolt (A) and remove the seat belt buckle (B).

8. Pull the seat belt switch harness (C) out through the space between the seat cushion and the seat linkage (driver's seat with manual height adjustable), or the hole on the seat track (driver's seat without manual height adjustable).
9. Install the buckle in the reverse order of removal and note these items:

- Assemble the washers on the centre anchor bolt as shown.
- If equipped with a side airbag, reconnect the negative cable to the battery.
- If equipped, enter the anti-theft code for the radio, then enter the customer's radio station presets.

1. TOOTHED LOCK WASHER
2. CENTRE ANCHOR BOLT
3. CENTRE ANCHOR
4. COLLER
5. SPRING WASHER