## Power Windows

#### Master Switch Replacement

22-200

4-door:

1. Remove the door grip cover (see page 20-7).
2. Remove the screws and power window master switch (A) from the door panel.

3. Disconnect the 20P connector (B) from the switch.
4. Remove the screws and switch (A) from the switch panel (B).

5-door:

1. Remove the door grip cover (see page 20-144).
2. Remove the screws and power window master switch (A) from the door panel.

3. Disconnect the 20P connector (B) from the switch.
4. Remove the screws and switch (A) from the switch panel (B).