## Front Pillar Outer Panel

#### Removal

3-17

- Cut the wheelhouse upper member as necessary, and cut and pry the front pillar outer panel.
- Check the front pillar lower stiffener position for damage, and replace it if necessary.
- When replacing the front pillar lower stiffener, remove the front pillar separator, and glue the insulator at the separator mounted position.

  1. FRONT PILLAR UPPER STIFFENER
  2. FRONT PILLAR LOWER STIFFENER
  3. OUTER PANEL
  4. SIDE SILL REINFORCEMENT
  5. FRONT PILLAR SEPARATOR
  6. INNER LOWER
  7. FRONT PILLAR LOWER STIFFENER
  8. FRONT PILLAR UPPER STIFFENER