## Interior Trim

#### Trim Removal/Installation - Quarter Pillar Area

20-207

NOTE:

- Put on gloves to protect your hands.
- When prying with a flat-tip screwdriver, wrap it with protective tape to prevent damage.
- Take care not to bend or scratch the trim and panels.

Remove the trim as shown.

Install the trim in the reverse order of removal and note these items:

- Replace any damaged clips.
- When installing the trunk side upper trim, slip the rear seat belt through the hole in the trim.
- Before installing the anchor bolt, make sure there are no twists or kinks in the belt.

  Fastener Locations
  A : Clip, 7 | B : Clip, 3 (White) | C : Clip, 1 | D : Clip, 2
  1. QUARTER PILLAR TRIM
  2. TRUNK SIDE TRIM PANEL
  3. REAR CENTRE SHELF
  4. TRUNK SIDE UPPER TRIM
  5. TRUNK SIDE UPPER TRIM
  6. BELT HOLE CAP
  7. REAR SEAT BELT
  8. REAR SEAT BELT LOWER ANCHOR BOLT, 7/16-20 UNF, 32 Nm (3.3 kgf m, 24 lbf ft)
  9. REAR DOOR SILL TRIM
  10. SEAT SIDE TRIM
  11. REAR DOOR OPENING TRIM