## Fuel and Emissions Systems

#### DTC Troubleshooting Index

11-314

Scan tool DTC | Honda DTC | Detection Item | Page
DTC | Temporary DTC | DTC (MIL Indication*) | Temporary DTC
P0107 | - | 3-1 (3) | - | Manifold Absolute Pressure (MAP) Sensor Circuit Low Voltage | (see page 11-359)
P0108 | - | 3-2 (3) | - | Manifold Absolute Pressure (MAP) Sensor Circuit High Voltage | (see page 11-360)
P0112 | - | 10-1 (10) | - | Intake Air Temperature (IAT) Sensor Circuit Low Voltage | (see page 11-361)
P0113 | - | 10-2 (10) | - | Intake Air Temperature (IAT) Sensor Circuit High Voltage | (see page 11-362)
P0117 | - | 6-1 (6) | - | Engine Coolant Temperature (ECT) Sensor Circuit Low Voltage | (see page 11-363)
P0118 | - | 6-2 (6) | - | Engine Coolant Temperature (ECT) Sensor Circuit High Voltage | (see page 11-364)
P0122 | - | 7-1 (7) | - | Throttle Position (TP) Sensor Circuit Low Voltage | (see page 11-365)
P0123 | - | 7-2 (7) | - | Throttle Position (TP) Sensor Circuit High Voltage | (see page 11-367)
P0131 | - | 1-1 (1) | - | Primary Heated Oxygen Sensor (Primary HO2S) (Sensor 1) Circuit Low Voltage | (see page 11-368)
P0132 | - | 1-2 (1) | - | Primary Heated Oxygen Sensor (Primary HO2S) (Sensor 1) Circuit High Voltage | (see page 11-369)
P0133 | P0133 | 61-1 (61) | T61-1 | Primary Heated Oxygen Sensor (Primary HO2S) (Sensor 1) Slow Response | (see page 11-370)
P0135 | - | 41-2 (41) | - | Primary Heated Oxygen Sensor (Primary HO2S) (Sensor 1) Heater Circuit Malfunction | (see page 11-371)
P0137 | P0137 | 63-1 (63) | T63-9 | Secondary Heated Oxygen Sensor (Secondary HO2S) (Sensor 2) Circuit Low Voltage | (see page 11-373)
P0138 | P0138 | 63-2 (63) | T63-9 | Secondary Heated Oxygen Sensor (Secondary HO2S) (Sensor 2) Circuit High Voltage | (see page 11-374)
P0139 | P0139 | 63-3 (63) | T63-9 | Secondary Heated Oxygen Sensor (Secondary HO2S) (Sensor 2) Slow Response | (see page 11-375)
P0141 | - | 65-2 (65) | - | Secondary Heated Oxygen Sensor (Secondary HO2S) (Sensor 2) Heater Circuit Malfunction | (see page 11-376)
P0171 | P0171 | 45-2 (45) | - | Fuel system Too Lean | (see page 11-378)
P0172 | P0172 | 45-1 (45) | - | Fuel system Too Rich | (see page 11-378)
P0300 and some of P0301 P0302 P0303 P0304 | - | 71-1 (71) 72-1 (72) 73-1 (73) 74-1 (74) | - | Random Misfire | (see page 11-379)

*: | These DTCs will be indicated by the blinking of the Malfunction Indicator Lamp (MIL) when SCS short connector is connected.
**: | The D indicator light and the Malfunction Indicator Lamp (MIL) may come on simultaneously.
*1: | D16W7, D16V1 engines
*2: | A/T
*3: | M/T