## Glass

#### Windshield Replacement (cont'd)

20-40

12. Glue the side rubber dams (A), lower rubber dam (B) and fasteners (C) to the inside face of the windshield (D) as shown:

- Be sure the rubber dam and fasteners line up with the alignment marks (E).
- Be careful not to touch the windshield where adhesive will be applied.

13. Glue the moulding (A) with adhesive tape (B) to the upper edge of the windshield (C):

- Be sure the alignment mark (D) of the moulding lines up with the alignment mark (E) of the windshield.
- Be careful not to touch the windshield where adhesive will be applied.

14. Install the fasteners (A) and retainers (B, C) to the body.

    Fastener Locations
    A: Fastener, 2 | B : Retainer, 2 | C : Retainer, 6