## Charging System

#### Alternator Overhaul (cont'd)

4-35

12. Remove the front bearing retainer plate.

13. Support the drive-end housing in a vice, and drive out the front bearing with a brass drift (A) and hammer.

14. With a hammer and the special tools, install a new front bearing in the drive-end housing.

Alternator Brush Inspection

15. Measure the length of both brushes with a vernier calliper.

- If either brush is shorter than the service limit, replace the rear housing assembly.
- If brush length is OK, go to step 16.

Alternator Brush Length:

Standard (New): | 19.0 mm (0.75 in.)
Service Limit: | 5 mm (0.2 in.)