## Standards and Service Limits

#### Fuel and Emissions

2-13

Item | Measurement | Qualification | Standard or New | Service Limit
Fuel pressure regulator | Pressure with fuel pressure gauge connected |  | 270-320 kPa (2.8-3.3 kgf/cm2, 40-47 psi)
Fuel tank | Capacity |  | 45 l (11.9 US gal, 9.9 Imp gal)
Engine idle for D14Z5, D16W7, D17Z1 engines (4-door model) | Idle speed with headlights and radiator fan off | M/T in neutral | 700+50 rpm (min-1)
A/T in or | 650+50 rpm (min-1)
Fast idle | M/T in neutral | 1,300+50 rpm (min-1)
A/T in or | 1,300+50 rpm (min-1)
Idle CO% |  | 0.1 max.
Engine idle for D15Y3, D17A5 engines (4-door model) | Idle speed with headlights and radiator fan off | M/T in neutral | 750+50 rpm (min-1)
CVT, A/T in or | 750+50 rpm (min-1)
Fast idle | M/T in neutral | 1,300+50 rpm (min-1)
A/T in or | 1,300+50 rpm (min-1)
Idle CO% |  | 0.5 max.
Engine idle for D15Y5, D15Y2, D16W8, D17Z1, D17Z2, D17Z5, D17A2, D17Z3 engines (4-door model) | Idle speed with headlights and radiator fan off | M/T in neutral | 720+50 rpm (min-1)
A/T in or | 720+50 rpm (min-1)
Fast idle | M/T in neutral | 1,300+50 rpm (min-1)
A/T in or | 1,300+50 rpm (min-1)
Idle CO% |  | 0.1 max.
Engine idle for D14Z5, D16W7 engines (5-door model) | Idle speed with headlights and radiator fan off | M/T in neutral | 700+50 rpm (min-1)
A/T in or | 650+50 rpm (min-1)
Fast idle | M/T in neutral | 1,300+50 rpm (min-1)
A/T in or | 1,300+50 rpm (min-1)
Idle CO% |  | 0.1 max.
Engine idle for D15Y5, D15Y2 D16W8, D17A1, D17Z1, D17Z2, D17Z5, D17A2, D17Z3 engines (5-door model) | Idle speed with headlights and radiator fan off | M/T in neutral | 720+50 rpm (min-1)
A/T in or | 720+50 rpm (min-1)
Fast idle | M/T in neutral | 1,300+50 rpm (min-1)
A/T in or | 1,300+50 rpm (min-1)
Idle CO% |  | 0.1 max.
Engine idle for D16V2 engine (5-door model) | Idle speed with headlights and radiator fan off | M/T in neutral | 750+50 rpm (min-1)
CVT, A/T in or | 750+50 rpm (min-1)
Fast idle | M/T in neutral | 1,300+50 rpm (min-1)
A/T in or | 1,300+50 rpm (min-1)
Idle CO% |  | 0.5 max.
Engine idle (Coupe model) | Idle speed with headlights and radiator fan off | M/T in neutral | 700+50 rpm (min-1)
A/T in or | 700+50 rpm (min-1)
Fast idle | M/T in neutral | 1,250+50 rpm (min-1)
A/T in or | 1,250+50 rpm (min-1)
Idle CO % | Except D17A5 engine | 0.1 max.
D17A5 engine | 1.0 max
Engine idle (5-door England made model) | Idle speed with headlights and radiator fan off | M/T in neutral | 700+50 rpm (min-1)
A/T in or | 700+50 rpm (min-1)
Fast idle | M/T in neutral | 1,250+50 rpm (min-1)
A/T in or | 1,250+50 rpm (min-1)
Idle CO % | Except D16V3 engine | 0.1 max.
D16V3 engine | 1.0 max

a a a