## Transmission Housing/Flywheel Housing

#### Start Clutch and Flywheel Housing Installation (cont'd)

14-383

21. Install the ATF pump drive sprocket (A) and put the ATF pump drive chain (B) on the ATF pump drive and driven sprockets, then install and tighten the three bolts.

22. Install the differential assembly (A).

23. Install the ATF passage line assembly (B) with the new O-rings (C).
24. Install the three dowel pins (D) and new flywheel gasket (E) on the transmission housing.
25. Install the flywheel housing (F) (20 bolts).
26. Install the ATF passage line holder assembly (G) with the new O-ring (H) (two bolts).