## Power Windows

#### Master Switch Test

22-194

1. Remove the power window master switch (see page 22-200).

2. Disconnect the 20P connector from the switch.

3. Disconnect the 20P connector (B) from the master switch.

Driver's Switch:

The driver's switch is combined with the control unit so you cannot isolate the switch to test it.

Instead, run the master switch input test procedures on page 22-190. If the tests are normal, the driver's switch must be faulty.

Front Passenger's Switch:

Left Rear Switch:

Right Rear Switch:

[ ] : RHD type

4. If the switch is faulty, replace the switch.