## Conventional Brake Components

#### Master Cylinder Disassembly

19-20

4-door

1. Remove the rod seal from the master cylinder (dual brake booster type) or brake booster (single brake booster type).
2. Remove the circlip (A) while pushing in the secondary piston (B).

3. Remove the reservoir (A).

4. On vehicle's with ABS, remove the stop pin (B) while pushing in the secondary piston (C).

5. Remove the piston guide (A) (dual brake booster type only), secondary piston (B) and primary piston (C).

6. Remove the reservoir seal (A) from the reservoir cap (B).

7. Remove the strainer (C) and grommets (D) from the reservoir (E).

NOTE: When the reservoir and master cylinder body are separated, replace the grommets with new ones.