## Seat Belts

#### Front Seat Belt Replacement (cont'd)

23-3

Install the belt in the reverse order of removal and note these items:

- If the threads on the retractor mounting self-tapping ET screw are worn out, use an oversized self-tapping ET screw made specifically for this application.
- Check that the retractor locking mechanism functions (see page 23-4).
- Assemble the washers, collars and bushing on the upper and lower anchor bolts as shown.
- Before installing the anchor bolts, make sure there are no twists or kinks in the front seat belt.
- Make sure the seat belt tensioner connector is plugged in properly.
- Reconnect the negative cable to the battery.
- If equipped, enter the anti-theft code for the radio, then enter the customer's radio station presets.

Upper anchor bolt construction:

1. BUSHING
2. UPPER ANCHOR
3. WASHERS
4. TOOTHED LOCK WASHER
5. COLLARS
6. SPRING WASHER
7. UPPER ANCHOR BOLT

Lower anchor bolt construction:

1. LOWER ANCHOR BOLT
2. TOOTHED LOCK WASHER
3. COLLAR
4. LOWER ANCHOR

Retractor bolt:

1. RETRACTOR BOLT
2. COLLAR
3. SPRING WASHER
4. TOOTHED LOCK WASHER
5. RETRACTOR