## Glass

#### Windshield Replacement (cont'd)

20-14

13. Glue the side rubber dams (A), lower rubber dam (B) and fasteners (C) to the inside face of the windshield (D) as shown:

- Be sure the rubber dams and fasteners line up with the alignment marks (E).
- Be careful not to touch the windshield where adhesive will be applied.

14. Glue the moulding (A) with adhesive tape (B) to the upper edge of the windshield (C):

- Be sure the alignment mark (D) of the moulding lines up with the alignment mark (E) of the windshield.
- Be careful not to touch the windshield where adhesive will be applied.

15. Install the fasteners (A), retainers (B, C) and clips (D) to the body.

A : Fastener, 2 B : Retainer, 2

C : Retainer,6 D : Clip, 2

a a a