## Engine Assembly

#### Engine Installation (cont'd)

5-20

37. Install the EVAP canister hose.

38. Install the shift cable (A) using the plastic washer (B), washer (C) and spring pin (D) (Honda multi matic).

39. Install the select cable (A) and shift cable (B) using the plastic washers (C), washers (D) and new cotter pins (E) (M/T).

40. Install the clutch slave cylinder (A) and clutch line bracket mounting bolt (B) (M/T).