## A/T Differential

#### Carrier Bearing Side Clearance Inspection (cont'd)

14-231

7. Measure the clearance between the 80 mm set ring and carrier bearing outer race with a feeler gauge.

STANDARD: 0-0.15 mm (0-0.006 in.)

8. If the clearance is out of standard, remove the 80 mm set ring and measure its thickness.
9. Select and install a new set ring, then recheck the clearance and make sure it is within the standard.

   SET RING, 80 mm

   No. | Part Number | Thickness
   1 | 90414-689-000 | 2.50 mm (0.098 in.)
   2 | 90415-689-000 | 2.60 mm (0.102 in.)
   3 | 90416-689-000 | 2.70 mm (0.106 in.)
   4 | 90417-689-000 | 2.80 mm (0.110 in.)
   5 | 90418-689-000 | 2.90 mm (0.114 in.)
   6 | 90419-PH8-000 | 3.00 mm (0.118 in.)