## SRS

#### General Troubleshooting Information (cont'd)

23-35

Reading the SRS Indicator Light Method (without service check connector (2P) models): The SRS indicator light indicates the DTC by the number of blinks when the DLC terminal box is connected to the Data Link Connector (DLC) 16P.

1. Make sure the ignition switch is OFF and wait for 10 seconds. Then connect the DLC terminal box (A) to the Data Link Connector (DLC) 16P (B). If you do not wait 10 seconds, the SRS unit will not be completely reset or output DTCs.

4-door

1. SRS INDICATOR LIGHT
2. JUMPER WIRE

5-door

1. SRS INDICATOR LIGHT
2. JUMPER WIRE

2. Connect the DLC terminal box terminals No. 4 and No. 9 with a jumper wire and push the operation switch.

3. Turn the ignition switch ON (II). The SRS indicator light comes on for about 6 seconds and then goes off. Then it will indicate the DTC.
4. Read the DTC.
5. Turn the ignition switch OFF and wait for 10 seconds. Then disconnect the DLC terminal box from the Data Link Connector (DLC) 16P.