## Doors

#### Door Glass and Regulator Replacement (cont'd)

20-10

3. Disconnect and detach the connector (A) and harness clip (B) from the door.

Fastener Locations

C : Bolt, 3D : Bolt, 4

4. Remove the bolts (C) and loosen the bolts (D), then remove the regulator (E) through the hole in the door. Power window is shown, manual window is similar.
5. Grease all the sliding surfaces of the regulator (A) where shown.

6. Install the glass and regulator in the reverse order of removal and note these items:

- Roll the glass up and down to see if it moves freely without binding.
- Make sure that there is no clearance between the glass and glass run channel when the glass is closed.
- Adjust the position of the glass as necessary.