## Mirrors

#### Rear-view Mirror Replacement

20-36

NOTE: When prying with a flat-tip screwdriver, wrap it with protective tape to prevent damage.

1. Using a flat-tip screwdriver, carefully remove the headliner cap (A) by releasing the hooks (B). Take care not to scratch the cap and headliner (C).

2. Remove the screws, then remove the rear-view mirror (A).

   Fastener Locations
   : Screw, 3

3. Install the mirror in the reverse order of removal.