## Seat

#### Rear Seat-back Cover Replacement (cont'd)

20-240

6. On right seat-back: If equipped with a centre shoulder belt, remove the screws, then remove the belt holder trim (A) and remove the trim from the centre belt (B).

Fastener Locations
: Screw, 2

7. Release the hooks (A) and unzip the seat-back cover (B). The right seat-back is shown, the left seat-back is similar.

8. On right seat-back: If equipped with a armrest, pass the armrest pivot (A) through the slit in the seat-back cover (B), then pull back the cover and release the hook strips (C).

9. Pull out the seat-back frame (A) from the pad (B), then pull out the headrest guides (C) while pinching the end of the guides and remove them. The right seat-back with middle headrest is shown, the right seat-back without middle headrest and the left seat-back are similar.

10. Remove the seat-back cover and pad from the seat-back frame. On right seat-back with centre shoulder belt, pass the centre belt (D) through the hole in the seat-back cover and pad.