## SRS

#### Driver's Airbag Replacement (cont'd)

23-166

Installation

1. Place the new driver's airbag (A) in the steering wheel and secure it with new Torx bolts (B).

4-door:

5-door:

2. Connect the cable reel 2P connector (A) to the driver's airbag 2P connector (B), then install the access panel (C) on the steering wheel.

4-door:

5-door:

3. Connect the battery negative cable.
4. After installing the airbag, confirm proper system operation:
   - Turn the ignition switch ON (II); the SRS indicator light should come on for about 6 seconds and then go off.
   - Make sure the horn button works.

5. Enter the anti-theft code for the radio, then enter the customer's radio station presets.