## Doors

#### Front Door Panel Removal/Installation - Manual Window (cont'd)

20-4

5. Remove the screws from the grip base (A) and door panel (B).

Fastener Locations

: Screw, 3

6. Release the clips that hold the door panel (A) with a commercially available trim pad remover (B), then remove the door panel by pulling it upward. Remove the door panel with as little bending as possible to avoid creasing or breaking it.

Fastener Locations

: Clip, 7

7. Install the door panel in the reverse order of removal and note these items:

- Replace any damaged clips.
- Make sure the rod is connected properly.
- Install the regulator handle so it points forward with the glass fully closed.