##

## General Information

#### Service Precautions (cont'd)

1-20

- Check for loose retainer (A) and rubber seals (B).

- The backs of some connectors are packed with grease. Add grease if necessary. If the grease is contaminated, replace it.

- Insert the connector all the way and make sure it is securely locked.
- Position wires so that the open end of the cover faces down.

Handling Wires and Harnesses

- Secure wires and wire harnesses to the frame with their respective wire ties at the designated locations.
- Remove clips carefully; do not damage their locks (A).

- Slip pliers (A) under the clip base and through the hole at an angle, then squeeze the expansion tabs to release the clip.

- After installing harness clips, make sure the harness does not interfere with any moving parts.
- Keep wire harnesses away from exhaust pipes and other hot parts, from sharp edges of brackets and holes and from exposed screws and bolts.
- Seat grommets in their grooves properly (A). Do not leave grommets distorted (B).