## Manual Transmission

#### Shift Lever Assembly/Disassembly/Reassembly

13-21

Prior to reassembling, clean all the parts in solvent, dry them and then apply lubricant to any contact surface.

1. SELECT LEVER
2. DUST SEAL

   Replace.

3. SELECT LEVER COVER
4. ROLLER
5. DUST COVER
6. OIL SEAL

   Replace.

7. BREATHER CAP
8. SHIFT ARM COVER
9. SELECT SPRING COLLAR
10. SELECT SPRING
11. SELECT SPRING PLATE
12. INTERLOCK
13. SHIFT ARM
14. 8 mm SPRING WASHER
15. 8 mm SPECIAL BOLT

    31 Nm (3.2 kgf/m, 23 lbf/ft)

16. SHIFT LEVER