## Engine Assembly

#### Engine Installation (cont'd)

5-16

1. Install the clutch slave cylinder (A) and clutch line bracket mounting bolt (B).

1. Install the battery cables (A) on the under-hood fuse/relay box, then install the harness clamp (B).

1. Install the ground cable (C).

1. Install the intake air duct.

1. Install the air cleaner housing (A) and connect the IAT sensor connector (B).

1. Install the breather hose (C).

a a a