## Conventional Brake Components

#### Master Cylinder Reassembly (cont'd)

19-25

7. On vehicle's with ABS; align the slot in the primary piston with the stop pin hole (A) by pushing the secondary piston (B) in and install the stop pin (C).

8. Install the reservoir (D) to the master cylinder.
9. Install the new circlip (A) while pushing in the secondary piston (B). Be careful not to scratched damage on the piston surface with the circlip the circlip edges.

10. Adjust the pushrod clearance (see page 19-29).
11. Apply recommended seal grease in the master cylinder seal set to a new rod seal, and install the seal onto the master cylinder (dual brake booster type) or brake booster (single brake booster type) (see page 19-18).