## Cylinder Head

#### Valve Clearance Adjustment (cont'd)

6-16
Crankshaft Pulley Removal and Installation

14. Rotate the crankshaft 180o counter-clockwise to bring No. 2 piston to TDC. The ''UP'' mark (A) should be on the intake side of the head.

15. Check and if necessary, adjust the valve clearance on No. 2 cylinder.
16. Install the cylinder head cover (see page 6-55).

Special Tools Required

- Socket, 19 mm, 07JAA-001020A
- Handle, 07JAB-0010200
- Pulley holder attachment, HEX 50 mm, 07JAB-0010400
- Pulley holder attachment, HEX 50 mm, 07MAB-PY30100

Removal

1. Hold the pulley with holder handle (A) and holder attachment (B).

With P/S:

With EPS:

2. Remove the bolt with a 19 mm socket (C) and breaker bar.