## Dashboard

#### Dashboard Removal/Installation (cont'd)

20-224

Driver's side:

4. From under the dash, disconnect the interior wire harness connector (A), driver's door wire harness connectors (B), side turn signal light connector (C) (for some models), antenna lead (D) (pillar antenna), clutch switch connector (E) (on MT model) and brake switch connector (F) and disconnect the floor wire harness connectors (G) and engine compartment wire harness connectors (H) from the under-dash fuse/relay box (I). On auto A/C model, disconnect the air hose (J).

Middle portion:

5. From the driver's side, disconnect the floor wire harness connectors (A) and on manual A/C, disconnect and detach the air mix control cable (B).

6. From the passenger's side, disconnect the combination sub harness connector (A) and A/C sub wire harness connectors (B) and on manual A/C, disconnect and detach the mode control cable (C).