## Doors

#### Door Latch Replacement (cont'd)

20-8

5. Pull the glass run channel (A) away as necessary and remove the bolts, then remove the centre lower channel (B) by pulling it downward.

Fastener Location

: Bolt, 1

6. Release the lock knob (A) from the knob bracket (B) and detach the inner handle rod (C) from the rod holder (D). Detach the harness clip (E) and disconnect (and detach) the actuator connector(s) (F).

Without Super Locking:

Without Super Locking: