## Design Specifications

#### (cont'd)

2-25

Item | Measurement | Qualification | Specification
ELECTRICAL RATINGS | Battery |  | 12 V-36 AH/5 hours
12 V-45 AH/20 hours
Starter |  | 12 V-0.8 kW, 1.0 kW
Alternator |  | 12 V-70 A
Fuses | Under-hood fuse/relay box | 80 A, 40 A, 30 A, 20 A, 15 A, 7.5 A
Under-dash fuse/relay box | 20 A, 15 A, 10 A, 7.5 A
Light bulbs | Headlight high beam | 12 V-60 W
Headlight low beam | 12 V-55 W
Front turn signal/Front side marker lights | 12 V-21 W/5 W
Front position lights | 12 V-5 W/3 CP (candlepower)
Side turn signal lights | 12 V-5 W
Rear turn signal lights | 12 V-21 W
Brake/Taillights/Rear side marker light | 12 V-21W/5 W
Rear fog light | 12 V-21 W
Taillights | 12 V-5 W
High mount brake light | 12 V-21 W
Back-up light | 12 V-21 W
License plate light | 12 V-3 CP
Ceiling light | 12 V-8 W, 5 W
Luggage area light | 12 V-5 W
Individual map light | 12 V-8 W
Spotlights | 14 V-8 W
Gauge light | 14 V-1.4 W
Indicator light | 12 V-1.12 W

a a a