## Manual Transmission

#### Transmission Removal (cont'd)

13-9

1. Place the transmission jack under the transmission and remove the transmission mounting bolts.

1. Remove the harness bracket (A), then remove the intake manifold bracket (B).

1. Remove the two front transmission mounting bolts.

1. Pull the transmission away from the engine until the transmission mainshaft clears the clutch pressure plate, then lower transmission on the transmission jack.

1. Remove the transmission rear mount (A) and the transmission rear mount bracket (B).

a a a