## Automatic Transmission

#### System Description (cont'd)

14-36

Power Flow (cont'd)

Position

- Hydraulic pressure is applied to the servo valve to engage the reverse selector with the countershaft reverse gear while the shift lever is in the position.
- Hydraulic pressure is also applied to the 4th clutch, then the 4th clutch engages the mainshaft reverse gear with the mainshaft.
- The mainshaft reverse gear drives the countershaft reverse gear via the reverse idler gear. The countershaft reverse gear drives the reverse selector, reverse selector hub and the countershaft.
- The rotation direction of the countershaft reverse gear is changed via the reverse idler gear.
- Power is transmitted to the final drive gear, which in turn drives the final driven gear.

NOTE: The illustration shows the 7-position transmission; 6-position does not have the sub-shaft and related parts.

1. TORQUE CONVERTER
2. 4TH CLUTCH
3. SUB-SHAFT
4. MAINSHAFT REVERSE GEAR
5. MAINSHAFT
6. COUNTERSHAFT
7. REVERSE SELECTOR
8. COUNTERSHAFT REVERSE GEAR
9. REVERSE SELECTOR HUB
10. SERVO VALVE
11. FINAL DRIVEN GEAR
12. FINAL DRIVE GEAR