## PGM-FI System

#### Primary HO2S Replacement

11-92

CKP Sensor Replacement

Special Tools Required O2 sensor wrench 07LAA-PT50101

1. Disconnect the primary HO2S 4P connector (A), then remove the primary HO2S (B).

1. Install the primary HO2S in the reverse order of removal.

1. Disconnect the CKP 3P connector.

1. Remove the CKP sensor (A).

1. Install the part in the reverse order of removal with a new O-ring (B).

a a a