## PGM-FI System

#### ECT Sensor Replacement

11-93

TDC Sensor Replacement

1. Remove the air cleaner (see page 11-126).

1. Disconnect the ECT sensor 2P connector.

1. Remove the ECT sensor (A).

1. Install the part in the reverse order of removal with a new O-ring (B).

1. Remove the air cleaner (see page 11-126).

1. Disconnect the TDC sensor 3P connector.

1. Remove the TDC sensor (A).

1. Install the part in the reverse order of removal with a new O-ring (B).

a a a