## Cylinder Head

#### Rocker Arms and Shafts Disassembly/Reassembly (cont'd)

6-36

NOTE:

- Identify parts as they are removed to ensure reinstallation in original location.
- Inspect the rocker shafts and rocker arms (see page 6-38).
- The rocker arms must be installed in the same positions if reused.
- When removing or installing the rocker arm assembly, do not remove the camshaft holder bolts. The bolts will keep the holders, springs and rocker arms on the shaft.
- Prior to reassembling, clean all the parts in solvent, dry them and apply lubricant to any contact points.
- Bundle the rocker arms with rubber bands to keep them together as a set.

D16W8 engine:

1. RUBBER BAND
2. INTAKE ROCKER ARM ASSEMBLY
3. INTAKE ROCKER SHAFT
4. COLLAR B
5. SPRING
6. TIMING PLATE
7. RETURN SPRING
8. COLLAR A
9. No. 1 CAMSHAFT HOLDER
10. EXHAUST ROCKER ARM A
11. Letter "A" is stamped on the rocker arm.
12. EXHAUST ROCKER SHAFT
13. Letter "B" is stamped on the rocker arm.
14. SPRING
15. EXHAUST ROCKER ARM B
16. No. 5 CAMSHAFT HOLDER
17. No. 4 CAMSHAFT HOLDER
18. No. 3 CAMSHAFT HOLDER
19. No. 2 CAMSHAFT HOLDER