## Valve Body

#### Main Valve Body Disassembly, Inspection and Reassembly

14-183

1. Clean all parts thoroughly in solvent or carburettor cleaner and dry them with compressed air. Blow out all passages.
2. Do not use a magnet to remove the check balls, it may magnetise the balls.
3. Check all valves for free movement. If any fail to slide freely, refer to Valve Body Repair (see page 14-181).
4. Replace the valve body as an assembly if any parts are worn or damaged.
5. Coat all parts with ATF during assembly.
6. Install the filter in the direction shown.

   1. CPB VALVE
   2. SPRING SEAT
   3. VALVE CAP CLIP
   4. VALVE CAP
   5. 1-2 SHIFT VALVE
   6. 2ND ORIFICE CONTROL VALVE
   7. CHECK BALLS, 8
   8. FILTER

      Replace.

      Install in this direction.

   9. MANUAL VALVE
   10. VALVE CAP
   11. ROLLER
   12. SERVO CONTROL VALVE
   13. MAIN VALVE BODY

       Inspect for scoring and damage.

   14. RELIEF VALVE
   15. SPRING SEAT
   16. MODULATOR