## Automatic Transmission

#### Shift Lever Disassembly/Reassembly

14-143

4-door Model

NOTE: The illustration shows the LHD with interlock system model; the other models are similar.

1. A/T GEAR POSITION INDICATOR PANEL LID
2. SCREW

   3 Nm (0.3 kgf/m, 2 lbf/ft)

   Apply non-hardening thread lock sealant.

3. SHIFT LEVER KNOB
4. A/T GEAR POSITION INDICATOR PANEL
5. SHIFT LEVER COVER
6. A/T GEAR POSITION INDICATOR PANEL BRACKET
7. BUSHING

   SILICONE GREASE

8. SILICONE GREASE
9. PARK PIN SWITCH
10. SILICONE GREASE
11. SHIFT LEVER BRACKET BASE
12. SHIFT LOCK SOLENOID
13. PLUNGER SPRING
14. SHIFT LOCK SOLENOID PLUNGER
15. SILICONE GREASE
16. SHIFT LOCK STOP
17. SHIFT LOCK RELEASE SPRING
18. SHIFT LOCK RELEASE
19. A/T GEAR POSITION INDICATOR PANEL LIGHT BULB