## Front Suspension

#### Knuckle/Hub/Wheel Bearing Replacement

18-11

Exploded View

1. WHEEL BEARING, Replace.
2. SNAP RING
3. 6 mm FLAT WASHER, Replace.
4. FLAT SCREW, 6 x 1.0 mm, 9.8 Nm (1.0 kgf/m, 7.2 lbf/ft)
5. SPINDLE NUT, 22 x 1.5 mm, 181Nm (18.5kgf/m, 134 lbf/ft), Replace.
6. BRAKE DISC
7. HUB

   Check for deformation, damage and cracks.

8. SPLASH GUARD

   Check for corrosion, deformation and damage.

   Replace if rusted.

9. KNUCKLE

   Check for deformation and damage.