## Damper/Spring Replacement

18-2

Exploded View

1. DAMPER MOUTING BASE

   Check for deformation.

2. SLF-LOCKING NUT

   12 x 1.25 mm

   44 Nm (4.5 kgf/m, 33 lbf/ft)

   Replace.

3. UPPER SPRING SEAT
4. BUMP STOP

   Check for weakness and damage.

5. DAMPER UNIT

   Check for oil leaks, gas leaks and smooth operation.

6. DAMPER SPRING

   Check for free length.

7. UPPER SPRING MOUTING CUSHION

   Check for deterioration and damage.

8. DAMPER MOUTING BEARING

   Check for smooth operation.

a a a