## Manual Transmission

#### Reverse Shift Fork Clearance Inspection

13-21

Shift Lever Clearance Inspection

1. Measure the clearance between the reverse idler gear (A) and the reverse shift fork (B) with a feeler gauge (C). If the clearance is more than the service limit, go to step 2.

   Standard:

0.20 - 0.59 mm (0.007 - 0.024 in.)

Service Limit:

1.3 mm (0.051 in.)

1. Measure the width of the reverse shift fork.

- If distance is not within the standard, replace the reverse shift fork with a new one.
- If distance is within the standard, replace the reverse gear with a new one.

Standard:

13.4 - 13.7 mm (0.527 - 0.539 in.)

1. Measure the clearance between shift lever (A) and the select lever (B) with a feeler gauge (C). If the clearance is more than the service limit, go to step 2.

   Standard:

0.05 - 0.25 mm (0.002 - 0.010 in.)

Service Limit:

0.50 mm (0.020 in.)

1. Measure the groove of the shift lever.

- If distance is not within the standard, replace the shift lever with a new one.
- If distance is within the standard, replace the select lever with a new one.

Standard:

15.00 - 15.10 mm (0.591 - 0.594 in.)

a a a