## Design Specifications

####

2-22

Item | Measurement | Qualification | Specification
DIMENSIONS | Overall length |  | 4,410 mm (163.0 in.)
Overall width |  | 1,695 mm (66.7 in.)
Overall height | without roof antenna | 1,440 mm (56.7 in.)
with roof antenna | 1,565 mm (61.6 in.)
Wheelbase (MPW condition) |  | 2,575 mm (101.4 in.)
Track (MPW condition) | Front | 1,472 mm (58.0 in.)
Rear | 1,490 mm (58.7 in.)
Ground clearance |  | 140 mm (5.5 in.)
Seating capacity |  | Five (5)
WEIGHT | Curb weight | M/T | 1,096-1,182 kg (2,416-2,606 lbs)
A/T | 1,123-1,208 kg (2,476-2,663 lbs)
CVT | 1,167-1,208 kg (2,573-2,663 lbs)
Max. permissible weight | European models | 1,575-1,635 kg (3,472-3,605 lbs)
ENGINE | Type | D14Z6 engine | Water-cooled, 4-stroke SOHC engine
D16V1 engine | Water-cooled, 4-stroke SOHC VTEC engine
Cylinder arrangement |  | Inline 4-cylinder, transverse
Bore and stroke | D14Z6 engine | 75 x 79 mm (2.95 x 3.11 in.)
D16V1 engine | 75 x 90 mm (2.95 x 3.54 in.)
Displacement | D14Z6 engine | 1,396 cm3 (85 cu in.)
D16V1 engine | 1,590 cm3 (97 cu in.)
Compression ratio | D14Z6 engine | 10.4
D16V1 engine | 9.4
Valve train | D14Z6 engine | Belt driven, SOHC 4 valves per cylinder
D16V1 engine | Belt driven, SOHC VTEC 4 valves per cylinder
Lubrication system |  | Forced wet sump, with trochoid pump
Oil pump displacement | at 6,000 engine rpm (min-1) | 36.4 litre (38.5 US qt, 32.0 Imp qt) per minute
Water pump displacement | at 6,000 engine rpm (min-1) | 130 litre (137 US qt, 114 Imp qt) per minute
Fuel required |  | UNLEADED gasoline with 95 research octane number or higher

a a a