## Seats

#### Rear Seat Armrest Replacement – Fixed Type

20-98

For some models: NOTE: Take care not to tear the seams or damage the seat covers.

1. Remove the seat-back (see page 20-96).
2. Remove the screws, and release the hooks (A), then remove the trunk pass-through cover (B).

   Fastener Locations
   A : Screw, 2

3. Remove the bolts, then remove the armrest (A).

Fastener Locations
: Bolt, 4

4. Remove the beverage holder (A) from the armrest (B).

5. Install the armrest in the reverse order of removal.