## Manual Transmission

#### Transmission Installation (cont'd)

13-13

20. Connect the starter cables (A) to the starter. Make sure that the crimped side of the ring terminal is facing out.

21. Connect the back-up light switch connector.

22. Apply Urea Grease UM264 (P/N 41211-PY5-305) to the end of the slave cylinder rod. Install the slave cylinder. Take care not to bend the clutch line.

23. Connect the transmission ground cable (A), then install the clutch line bracket (B).

24. Install the intake air duct (A) and the air cleaner housing (see page 11-146).