## Bumpers

#### Front Bumper Removal/Installation

20-104

NOTE:

- Have an assistant help you when removing and installing the front bumper.
- Take care not to scratch the front bumper and body.
- Put on gloves to protect your hands.

Remove the front bumper as shown.

Install the bumper in the reverse order of removal, and note these items:

- If equipped, make sure the front fog light connector is plugged in properly, and the headlight washer tube is connected properly.
- Make sure the front bumper engages the hooks of the side spacers and upper beams on both sides securely.
- Replace any damaged clips.

  Fastener Locations
  A: Screw, 2 | B : Screw, 2 | C: Bolt, 4 | D : Clip, 8 or 10 | E : Clip, 2
  1. ABSORBER

     (For some models)

  2. HOOKS
  3. HOOKS
  4. SIDE SPACER
  5. UPPER BEAM
  6. FRONT INNER FENDER
  7. WASHER TUBE

     (For some models)

  8. FRONT BUMPER

     If equipped, disconnect the front fog light connector and the headlight washer tube.

  9. Without front air spoiler.
  10. FRONT AIR SPOILER

      (For some models)

  11. AIR SPOILER PLATE
  12. PLATE
  13. SPOILER
  14. BUMPER
  15. Without front air spoiler